Transmitter section Early Warning System For hazardous condition using wireless sensor

XBEE

Vcc Gnd Tx Rx

Vcc

Gnd

O/p

Smoke Sensor

Vcc Gnd 10 11 9 8

Arduino

Vcc Gnd O/P

GSM Module

Receiver section of Early Warning System For hazardous condition using wireless sensor



Vcc Gnd 10 11 12

Arduino

XBEE

Vcc Gnd TX Rx